PURE **STOCK FARM CLASS RULES**

 **2023**

**9700 # STOCK 12,700# STOCK**

 **10,700 # STOCK 13,700# STOCK**

 **11,700# STOCK**

 **1. All stock classes must be stock and out of the field. Must be stock block or its factory replacement. Turbo are optional.

2. Rubber tires only. NO cut tires, No tire studs, NO chains, NO 4-wheel drives or front wheel assists. Tire size is 20.8 X 38 to 18.4 X 42. No aluminum rear rims. Cast or steel rear rims only.

3. *MPH Limit*:**

 **9700 # class 6 MPH 12,700# class 6 MPH**

 **10,700 # class 6 MPH 13,700# class 6 MPH**

 **11,700# class 6 MPH**

 **Disqualification if warning is given AFTER 100 ft. mark for being over MPH**

 **limit.

4. All tractors must have functioning hydraulics and PTO.(If factory equipped.)
 Must have operational rock shaft housing. If tractor has no rock shaft must have**

 **Factory plate.**

**5. NO CURVED STACKS ALLOWED. Straight pipe only. Must have factory**

 **Muffler to have curved pipe.

6. No inline pumps unless factory equipped. Stock factory pump on stock block for**

 **That particular model tractor.

7. Maximum engine speed of stock RPMS, according to Nebraska Test Manual.**

 **Allowance of 10 RPMS. All tractors are subject to a random RPM check at**

 **Time by a rules committee member. Disqualification if over allowed RPMS for**

 **That class.**

 **8. All tractors must be data logger equipped. (non members do not need the data**

 **Logger equipment.)**

 **9. Non Members will be allowed 4 hooks or 2 events. After the 2 events the puller**

 **Will be required to be a member and be data logger equipped. Non members**

 **Will be required to have wheelie bars after their 4 hooks or 2 events.**